|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Router ID (8bit) - Sender | | | | | | | |
| Node ID (8bit) - Receiver | | | | | | | |
| The sixth code of Pipe (Sender) | | | | | | | |
| The fifth code of Pipe (Sender) | | | | | | | |
| The fourth code of Pipe (Sender) | | | | | | | |
| Hopcount (8byte) | | | | | | | |
| Protocol (7 bit) | | | | | | | Flags |
| Fragment offset (5bit) | | | | | Data length (3bit) | | |
| Checksum7 | Checksum6 | Checksum5 | Checksum4 | Checksum3 | Checksum2 | Checksum1 | Checksum0 |
| Data0 | | | | | | | |
| Data1 | | | | | | | |
| Data2 | | | | | | | |
| Data3 | | | | | | | |
| Data4 | | | | | | | |
| Data5 | | | | | | | |
| Data6 | | | | | | | |
| Data7 | | | | | | | |
| 8 \* 3 = 24 bit (optional) – for developer | | | | | | | |